BMS FILES FOR F65540/545:

Panels:

(1)  MONODD.BMS		;640x480 Dual Scan Monochrome (Default)
			;(Sharp LM64P80)
(2)  MONODDEX.BMS	;640x480 Dual Scan Monochrome using external
			;buffer (Sharp LM64P80) 
(3)  MONODDNA.BMS	;640x480 Dual Scan Monochrome using external
			;buffer & No Accelerator (Sharp LM64P80) 
(4)  STNDD.BMS		;640x480 Color STN DD -8/16 Bit Interface
			;(Sharp LM64C08)
(5)  STNDDEX.BMS	;640x480 Color STN DD -8/16 Bit Interface
			;Using external buffer (Sharp LM64C08)
			;for 2-DRAM Memory Configuration.
(6)  STNDDNA.BMS	;640x480 Color STN DD -8/16 Bit Interface
			;Using external buffer & No Accelerator 
			; (Sharp LM64C08)
(7)  STNDD1DR.BMS	;640x480 Color STN DD -8/16 Bit Interface
			;(Sharp LM64C08)
			;for 1-DRAM Memory Configuration.
(8)  TFTCLR.BMS		;640x480 Color TFT With Display Enable
			;(Sharp LQ9D011, Toshiba LTM09C015-1)
(9)  HTCTFT.BMS		;640x480 Color TFT
			;(Hitachi 26DS2, Hitachi TX26D02VC2AA)
(10) 1Kx768TFT.BMS	;1024x768 Color TFT
			;(Sharp LQ10dx01)
(11) 18BTFT.BMS		;640x480 Color TFT 18-Bit Interface
			;
(12) STN4BIT.BMS	;640x480 4-Bit Pack STN Color
			;(Sanyo LCM5327-24NAK, LM-CK33-33-22NEZ,
			;LCM 5330)
(13) STNE4BIT.BMS	;640x480 4-Bit Extended Pack STN Color
			;(Sharp LM64C031)
(14) ELDD640.BMS	;640x480 EL DD
			;(Sharp LJ64H052)
